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Section 5 – Scope of Works 
This Section contains the Specifications, the Drawings, and supplementary information that describe the Works to be procured.
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Specifications (Refer Separate Volume)
Drawings (Refer Separate Volume of Drawings)
Bill of Quantities

PART A: Bill of Quantities (BOQ)

PART B: Day Works

Supplementary Information

The Multipurpose Hall and Play Ground is located within the premises of Nepal Administrative Staff College, Jawalakhel, Lalitpur, Nepal. The land, owned by the NASC
There are basically different types of building structures used for different proposed like administration, library, training hall, hostel etc.  

Construction of Multipurpose Hall, Changing Room, Toilet, Football Ground and Facility Improvement of Existing Basket Ball, Volley Ball and Badminton Court:  
New structure for Multipurpose Hall, Changing Room and Toilet should be constructed on open space as shown in the Master Plan. For exterior and interior walls are brick, prefab board and cement board. Flooring works in room for changing and multipurpose hall are neat cement punning and in toilet tile flooring is proposed. For elevation treatment clay brick tile cladding in wall and ACP is used for cornice. For walkway PPC is proposed. The roofing sheet should be Trapezoidal CGI color sheet brown in color with metal truss and punning. For Existing Basket Ball, Volley Ball and Badminton Court, the existing facility needs to be improved by PCC and PVC work. 
1. Construction of Play Ground
Dubo Grass is used in football playground and brick dust is used for running track. The viewing area and circulation area, PCC flooring is proposed. 3” thick PCC flooring over existing PCC is proposed in existing playground (badminton and basketball court). PVC flooring is proposed in volley ball court, remaining circulation flooring should be PCC.   
2. Provision of Drainage

Covered drain been provided along the periphery of the central platform to collect run-offs from the structure and the pavement. The water thus collected shall be discharged to the existing man hole as shown in drawing.

